DIXIE ROAD
Composer:	Dennis & Ginny  Crapo, 7331 Ridgemont Dr. SE. Olympia,  Wa.  98503
Record:		 MCA 52664?    “Dixie Road” by Lee Greenwood		Rhythm/Phase:	Two-Step     II
Footwork:	Opposite, directions for the man except where noted
Sequence:	 INTRO, A, A, B, B, BRIDGE, A, B, B, C, C, ENDING
      EDDIE’S & BOBBIE’S RECORDS
         INTRO			                                 1835 SO BUCKNER
1-4		WAIT; WAIT; APTY, -; PT, -; TOG(CP/WALL), -; TCH, -;		      P. O. BOX 17663
1-4	In open fcg pos M fcg wall wait two meas;; standard ackn to CP M fcg wall;; 			         DALLAS, TEXAS 75217
5-8		TRAVELLING BOX::::
	5-8	Sd L twd LOD, cl R to L,  fwd L twd wall, -; (fc RLOD in RSCP) fwd R, -, L, -;(CP/WALL)
Sd R twd RLOD, cl L to R, bwd R twd COH, -; (SCP/LOD) fwd L, -, pkup R, (CP/LOD), -;
PART A
1-4		(CP/LOD) FWD TWO STEP; FWD TWO STEP; PROG SCISS {SCAR}; PROG SCISS BJO);
1-4	2 fwd two steps L, R, L, -: R, L, R, -; sd L twd COH, cl R to L, XLIF of R(W XIB) to SCAR/DLW, -;
sd R twd wall, -, cl L to R, XRIF of L(W XIB} to BJO/LOD, -;
5-8		(BJO/LOD) FWD LOCK FWD; FWD LOCK FWD; (CP/WALL) TURN TWO-STEP;
TURN TWO-STEP;
5-6	fwd L. lock RIB of L(W LK IF), fwd L, -; fwd R, lock LIB of R(W LK IF), fwd R trn ¼ RF to CP/WALL,.-;
7-8	sd L twd LOD, cl R to L, fwd L trn ½ RF to LOP/COH, -; sd R twd LOD cl L to R, fwd R trng RF ½ to end 
in BFLY/WALL, -;
9-12		(BFLY/WALL.) FC TO FC; BK TO BK; BASKETBALL TURN;;  (OP/LOD)
9-10	sd L twd LOD, cl R to L, sd L trng away to bk to bk, .-; sd R twd LOD, cl L to R, sd R trng to OP/LOD, -;
11-12	lunge LOD L trng  ¼ RF, -, rec R trng ½ RF to LOP/RLOD, -; lunge RLOD L trn ¼ RF, -, rec R trng ¼ RF 
ending OP/LOD, -;
13-16		(OP/LOD) HITCH SIX;; (BFLY/WALL) SD, CL, .SD, CL; (SCP/LOD) WALK, -, PKUP, -;
(CP/LOD)
13-14	fwd L, cl R to L, bk L, -; bk R, cl L to R, fwd R trng ¼ to BFLY/WALL, -;
15-16	sd L, cl R to L, sd L, cl R to L; fwd L trng ¼ to SCP/LOD, -, pkup R, -;
2nd & 3rd time  thru part A meas 16, fwd L trng to OP/LOD, -, fwd R, -;
PART B
1-4		(OP/LOD) {SLIDING DOOR) RK SD, -, REC, -; X, SD X, -; RK SD, -, REC, -;  X, -, SD, X, -;
1-4	rk sd L twd COH, -, rec R twd wall, -; XLIF of R, sd R, -, XLIF of R, .-;
rk sd R twd wall, -, rec L twd COH, -; XRIF of L, sd L, -, XRIF of L, .-;(OP/LOD)
5-8		(OP/LOD) HITCH FOUR; WALK TWO TO FC(CP WALL); TURN TWO STEP;
TURN TWO STEP;
5-6	fwd L, cl R to L, bk L, cl R to L;  fwd L, -, fwd R trng ¼ to CP/WALL, -;
7-8	repeat meas 7-8 of part A en4ing in OP/LOD;;
 2nd time thru part B end in BFLY/WALL; 4th time thru part B end in CP/LOD.
BRIDGE
1-2		APT, -, PT, -; PICKUP, -, TCH(CP/LOD), -;
1-2	(CP/WALL)step apt L to fc LOD, -, pt R twd LOD, -; pkup R(CP/LOD), -, tch L to R, -;
PART C
1-4		TWIST VINE, -, 2, -; HALF BOX FWD; TWIST VINE, -, 2, -; HALF BOX FWD(turn ½ R);
1-2	(CP/LOD)sd L twd COH, -, XRIB of L(W XLIF) to momentary SCAR, -; blend to CP/LOD sd L twd COH,
 cl R to L, fwd L twd LOD, -;
3-4	sd R twd wall, -, XLIB of R(W XRIF) to momentary BJO, -; blend to CP LOD sd R twd wall, cl L to R,
 fwd R trng ¼ RF BFLY/WALL, -;
5-8		 (BFLY/WALL)TWIRL VINE, -; SD TWO STEP; REV TWIRL VINE, -, 2, -; SD TWO STEP;
5-8	sd L twd LOD, -, XRIB of L(as W twirls RF under joined lead hands R, .-, L, -;) to BFLY/WALL.-;
sd L twd LOD, cl R to L. sd L, -; sd R twd RLOD, -, XLIB of R (as W twirls LF under joined lead hands
L, -, R, -;) to BFLY/WALL.-; sd R twd RLOD, cl' L to R,  sd R twd RLOD, -;
9-12		(BFLY/WALL) AWAY, STEP, STEP, -; TOG, STEP, STEP, -; AWAY, STEP, STEP, -; TOG, STEP,. 
STEP, -;
9-10	fwd L trng slightly bk to bk, step R, step L, -; fwd R trng to fc ptr & wall, step L, step R; -,
11-12	repeat  meas  9-10 part C to BFLY/WALL;;
13-16		SLOW OPEN VINE; ; TURN TWO STEP; TURN TWO STEP;
13-14	sd L twd LOD trng slightly RF, -, XRIB of L to LOP/RLOD, -; sd L twd LOD trng to fc ptr & wall 
momentarily, -, thru & fwd R twd LOD blend to CP/WALL, -;
15-I6	repeat  meas 7-8 of part A ending in CP/LOD;;
2nd time thru part C end in CP WALL:
ENDING
1-4	 	(CP WALL) TRAVELING BOX;;|;;
1-4	repeat meas 5-8 of the introduction ending in SCP/LOD;;
5-8		SD, CL, SD, .CL; APT, -, PT, -;
5-8	blend to BFLY/WALL sd L twd LOD, cl R to L, sd L twd LOD, cl R to L; step apart L ,-, point R twd ptr, -;