I DON'T WANT TO BE ME
Composer:	Dort & Les Fuhrman, 1277 S.Meridian Rd., Mason, MI.,48854
Record:		ENO14 (HH 945)
Rhythm/Phase:	Two Step/ III
Footwork:	Opposite throughout, directions for M unless otherwise stated
Sequence:	Intro, A, B, Interlude C, B, Ending

INTRO
1-4		WAIT; WAIT; HITCH 4; WALK PICKUP;
1-2	OP LOD wait; wait;
3-4	Fwd L, cl R, bk L, cl R; fwd L, -, fwd R picking W to CP LOD, -;

PART A
1-4		TWO FWD TWO STEPS;; POINT SIDE, STEP, STEP, -; SCIS SCAR;
1-2	CP LOD fwd L, cl R, fwd L, -; fwd R, cl L, fwd R, -;
3-4	Point L twd COH, step in place L, step in place R, -; aide L, cl R, XLIF (W XRIB) to SCAR DLW, -;
5-8		PT FWD, -, PT BACK, -; RUN 3 CP LOD; PT FWD, -, PT BACK, -; RUN 3;
5-6	Point fwd R, -, point bk R, -; fwd R, L, R to CP LOD, -;
7-8	Point fwd L, -, point bk L, -; fwd L, R, L,-;
9-12		TWO FWD TWO STEPS;; POINT SIDE, STEP, STEP, -; SCIS BJO;
9-10	CP LOP fwd R, cl L, fwd R, -; fwd L, cl R ,fwd L, -;
11-12	Point R twd WALL, step in place R, step in place L,-; sd R, cl L, XRIF (W XLIB) to BJO/LOD, -;
13-16		PT FWD, -,PT BK, -; RUN 3 CP LOD; PT FWD, -,PT BK, -; RUN 3 VARS LOD SAME FOOTWORK;
	13-14	Point fwd L, -, point bk L, -; fwd L, R, L to CP LOD,-;
15-16	Point fwd R, -, point bk R, -;  fwd R, L, R {W turn RF R, fwd L, touch	L to. VARS LOD),-;

PART B
1-4		PT FWD, -, PT BK, -; CROSS, SD, FWD, -; PT FWD, -, PT BK, -; CROSS, SD, FWD, -;
1-2	(Same footwork)VARS LOD point fwd L, -, point bk L, -; XLIB, sd R, fwd L, -;
3-4	Point fwd R, -, point bk R, -; XRIB, sd L, fwd R, -;
5-8		WALK    2;    FWD, LOCK, FWD, -; STAIRS 4; WALK    TOUCH;
	5-6	Fwd L, -, fwd R, -; fwd L, lk R in bk, fwd L, -;
7-8	Sd R, cl L, fwd R, cl L; fwd R, -, touch L, -;
9-12		HITCH 4; TURN ¼LF, -, CL, -; HITCH 4; TURN ¼LF, -,CL, -;
	9-10	Fwd L, cl R, bk L, cl R; fwd L turning  ¼LF to fc COH, -,cl R, -;
11-12	Fwd L, cl R, bk L, cl R; fwd L trn ¼LF to fc RLOD, -,cl R, -;
13-16		HITCH 4; TURN ¼LF, -, CL, -; HITCH 4; SD, -, CL TRANSITION TO BFLY WALL, -;
13-14	Fwd L, cl R. bk L, cl R; fwd L trng ¼LF to fc WALL, -; 
15-16	Fwd L, cl R, bk L, cl R; sd LOD L,-, cl L (W L trng LF to BFLY WALL, -, touch R), -;

INTERLUDE
1-4		SIDE, CLOSE, SIDE, CLOSE; SIDE, -, THRU, -; SIDE, CLOSE, SIDE, CLOSE; WALK PICKUP;
1-2	BFLY WALL sd LOD L, cl R, sd L, cl R; sd L, -, thru R, -;
3-4	Sd L, cl R, sd L, cl R; blending to SCP LOD 	fwd L, -, fwd R picking W up to CP LOD, -;

PART C
1-4		PROGRESSIVE SCIS BJO CHECK;; WHALETAlL;;
1-2	CP LOD sd L cl R, XLIF(W XRIB)to SCAR DLW, -) sd R, cl L, XRIF(W XLIB)to BJO LOD ck fwd motion, -; 
3-4	XLIB, sd R, fwd L, lk R in bk; sd L, cl R, XLIB, sd R;
5-8		FWD LOCK FWD TWICE;; WALK 4 TO BFLY WALL;;
	5-6	BJO LOD fwd L, lk R in bk, fwd L, -; fwd R, lock L in bk, fwd R, -;
7-8	Fwd L, -, fwd R, -; fwd L, -, fwd R to BFLY WALL, -;
9-12		ROCK SIDE, -, REC, -; CROSS, SIDE, CROSS, -; ROCK SIDE, -, REC OP LOD, -; FWD TWO STEP;
	9-10	BFLY WALL rk sd LOD L, rec R, -; XLIF, sd R, XLIF, -;
11-12	Rk sd RLOD R, rec L to OP LOD, -; fwd R, cl L, fwd R, -;
13-16		SLIDING DOOR;; SLIDING DOOR TRANS VARS LOD;;
13-14      OP LOD rk sd COH L, -, rec R, -; XLIF, sd R, XLIF (W change sides IF M to LOP LOO).-;
15-16	Rk sd WALL R, -, rec L, -; XRIF, sd L. XRIF (W change sides IF M XLIF, sd R, touch L) to VARS LOD, -;

ENDING
1-4		SIDE, CLOSE, SIDE, CLOSE; SIDE, -, THRU, -; SIDE, CLOSE, SIDE, CLOSE; APART, -, POINT, -;
	1-4	Repeat measures l thru 3 of INTERLUDE;;; step apart from ptr L, -, point R, -;