MORE
Composer:	Ivan & Billie Sager, 2620 Purdue Ave., Los Angeles, Ca. 90064
Record:		POLYDOR HVG533    Kai Wlndlng Orch.			Slow to 42-43
Rhythm/Phase:	Fox-Trot
Footwork:	Opposite throughout, directions for M unless otherwise stated
Sequence:	INTRO, A, A, B, C, B, A, B, ENDING.

INTRO	
1-4		OP DLW WAIT; APT, -, PT, -; IN PLACE R, L, R(W SPIN); SWAY L & R;
	1-2	Wait 1 meas in OP M fcg DLW Apt L, -, pt R twd ptr, -;
	3-4	M step in plc R, L, R, (W spot spin LF L, R, L to CP)-; sway L, tch R, sway R, tch L;
PART A
1-4		CP WALL WHISK; THRU FAN, -, CUT, BK; CUT, -, BK, CL; PICK UP, -, SD, CL;
	1-2	Fwd L, -, sd & fwd R rising(W trn VSCP), XLIB(W XIB); lower & step thru on R & fan L CW(W CCW), 
-, cut L in front of R, bk R;
	3-4	In SCP cut L in front of R, -, bk R, cl L; fwd R pkup, -, sd L, cl R;
5-8		CP/DLC FWD L, -, SD, BK; BK, -, FWD, SD; BK, BK, SD,  FWD; FWD, -, FWD, -;
	5-6	Fwd L, - begin LF trn, sd R fc COH(W heel trn), bk L fc DLC; bk R, - with ck action to start weave, fwd L 
RLOD, sd R COH;
	7-8	Cont weave bk L DC, bk R DC, sd L trng LF DW , fwd R BJO DW; fwd L, -, R blend CP WALL, -;

PART B
1-4		CP WALL FWD, -, TRN, BK; BK, -, 2, 3; BK, -(W swivel), FWD R, -; VINE 4 MANUV;
1-2	Fwd L, -, sd R trng  ¼LF BJO, bk L RLOD; bk R, -, L, R;
3-4	Bk L RLOD brush R across L, -, rec R, (W fwd R & flare L trng RF to SCP, -, fwd L,)-; blend CP/WALL sd 
L, XRIB (W XIB), sd L, XRIF Manuv ;
5-8		CP RLOD PIVOT, 2,  TWL, 2; FWD, -, CK, -; FISHTAIL; FWD, -, FWD, -;
5-6	CP RLOD RF couple piv L, R fc LOD, fwd L, R(W RF twl R, L to OP); OP LOD fwd L, -,R ck, -;
7-8        OP fishtail XLIB of R, sd R, fwd L, lk R(W XRIBL, sd L, fwd R, lk L); fwd L, -, R BFLY/WALL, -;
Note: 2nd Time Only Thru Part B End In Cp Wall

PART C
1-4		BFLY WALL RK SD, -, REC, CROSS; RK SD, -, REC, CROSS; RK SD, -, REC, CROSS; OP RLOD 
FWD, -, FWD/LK, FWD;
1-2	BFLY/Wall rk sd L LOD, -, rec R, XLIFR(W XIF); rk sd R RLOD, -,rec L, XRIFL(W XIF);
3-4	Repeat meas 1 of PART C; blend L OP fc RLOD fwd R, -, fwd L/lk R, fwd L;
5-8		BFLY WALL RK SD, -, REC, CROSS; SD, -, BHND, SD; CROSS, -, SD, BHND; CP WALL RK
SD, -, SD/CL, SD;
5-6	BFLY/WALL repeat meas 2 PART C; sd L, -, XRIBL (W XIBR), sd L;
7-8	XRIFL(W XIFR) ,-, SD L, XRIBL(W XIBR); blend CP WALL rk sd L, -, rec R/sl L, sd R;

ENDING
1-5		BFLY WALL RK SD, REC, CL, -, RK SD, REC, CL, -; TRN OUT, -, PT, -;TRN	IN, -, PT, -; APT, -,  PT, -;
	1-2	BFLY/Wall rk sd L, rec R, cl L, -; Rk sd R, rec L, cl R,-;
	3-5	Sd L LOD trng out to bk to bk pos, -, pt R LOD, -; sd R LOD trng RF to BFLY, -, pt L LOD,  -; Apt L,-,pt 
R twd ptr, -;